    The Project Gutenberg EBook of The Art of Graining: How Acquired and how
    Produced., by Charles Pickert and A. Metcalf

    This eBook is for the use of anyone anywhere at no cost and with
    almost no restrictions whatsoever.  You may copy it, give it away or
    re-use it under the terms of the Project Gutenberg License included
    with this eBook or online at www.gutenberg.org

    Title: The Art of Graining: How Acquired and how Produced.
           With the description of colors and their applications.

    Author: Charles Pickert
            A. Metcalf

    Release Date: March 8, 2014 [EBook #45079]

    Language: English

    Character set encoding: ISO-8859-1

    *** START OF THIS PROJECT GUTENBERG EBOOK THE ART OF GRAINING ***

    Produced by Chris Curnow, Mary Akers and the Online
    Distributed Proofreading Team at http://www.pgdp.net (This
    file was produced from images generously made available
    by The Internet Archive)

Transcriber's note:
Minor spelling and punctuation inconsistencies been harmonized. Obvious printer errors have been repaired. Missing page numbers are page numbers that were not shown in the original text. Please see the end of this book for further notes.

# THE
ART OF GRAINING:
HOW ACQUIRED AND HOW PRODUCED.

WITH

DESCRIPTION OF COLORS

AND

THEIR APPLICATIONS.

WITH

LITHOGRAPHIC ILLUSTRATIONS

OF

THE VARIOUS WOODS USED IN INTERIOR FINISHING.

WITH 42 COLORED PLATES ON STONE.

BY

CHARLES PICKERT AND A. METCALF.

NEW YORK:
D. VAN NOSTRAND, PUBLISHER, 23 MURRAY AND 27 WARREN STREET.
1872.

Entered according to Act of Congress, in the year 1872, by
CHARLES PICKERT AND A. METCALF,
in the Office of the Librarian of Congress at Washington.

## INTRODUCTION.

The Art of Graining is judged by the authors of this treatise to be of sufficient importance to justify a work devoted especially to the task of giving instruction to learners of the art.

All graining is an imitation of some more or less well known wood, and the learner may doubtless draw from nature the copies he desires to imitate; but it is only trained skill that can accomplish the task perfectly, and it is presumably true that those who, in acquiring a long experience, have made the obstacles to success a special study, are best prepared to afford instruction to a beginner.

The authors of the work present here the result of a long experience in the practice of this decorative art, and feel confident that they hereby offer to their brother artisans a reliable guide to improvement in the practice of graining.

It is earnestly recommended by the authors that learners should practise drawing the several copies given as samples, with drawing pencils, using both narrow and broad-pointed, as the surest means of acquiring such thorough mastery of proper manipulation as will insure the highest degree of success.

It is believed, moreover, that experienced learners will find it not amiss to avail themselves of the methods set forth in this treatise, affording as they do, the sum of the examples of fellow-artisans who have carefully 4 studied nature's own modes, and have studiously followed such plans in working as insured the closest and most durable adherence to the original form and color.

CHARLES PICKERT,
A. METCALF.

## INSTRUCTIONS

HOW TO MIX AND APPLY THE COLORS IN GRAINING THE VARIOUS WOODS HEREIN REPRESENTED.

As oak and black walnut are the principal woods imitated in graining, we have given them a prominent place and careful attention in our work, for when the ability to produce imitations of those properly is once thoroughly attained, the graining of other woods becomes a comparatively easy task.

First:—In preparing work for graining, great attention should be given to the shellacking of all knots and other parts containing any inequalities of surface, whether from the exudation of pitch, gum, or other substance; unless this precaution is observed the pitch or gum will force itself through a great many coats of paint.

6

## OAK.

Illustrations of OAK include Plates 1-17.

For oak-graining the priming coat should be white, mixed (not too thickly) with pure lead and linseed-oil; then, when thoroughly dry, and ready for a second coat of paint, much care should be observed in well stopping or puttying with white lead or common putty, as may be thought best, leaving all nail-holes or other inequalities well filled, pressed in and rounded up, so that when thoroughly sand-papered it will leave the surface entirely smooth and level. For a second coat of paint, a little yellow chrome or Rochelle may be added, sufficient to make it a light cream color, using for a body pure lead, turpentine, oil, and a small quantity of japan, making the paint a trifle thicker than the priming coat, having it well mixed and strained, so that it shall not contain any lumps or foreign substance. Here let us say that the habit of undertaking to do graining work on two coats of paint is entirely wrong; good work cannot by any possibility be performed unless there shall have been at least three coats laid on as a foundation,—otherwise it will not wipe out clean, but will appear muddy and foul when completed.

For a third coat of grained work, if a very light oak is desired, add to the same mixture of lead, oil, etc., sufficient yellow as before, to produce a delicate cream, adding to that a very small quantity of American vermilion, or Venetian red. After laying on the second coat, the work should be well and carefully sand-papered, puttying (as before suggested), if necessary. When the third coat has been on two or more days, and has become thoroughly hard and dry, use upon the surface very fine sand-paper, so that a perfectly smooth finish may be obtained.

7 For light-oak graining-color, use equal parts of raw umber and raw Sienna, and if a little darker shade is desired, tone with burnt umber, grinding into the same a little Paris, or common whiting, which gives it body and holds it together. A little beeswax or brown Windsor soap dissolved in turpentine may be used if desired, but in a small quantity.

For mixing the colors employ one-fourth boiled oil, three-fourths turpentine, adding for drier a very little japan. Graining-colors should invariably stand from six to ten hours after mixing before being applied, and if too thick, when adding the thinners be cautious to avoid stirring from the bottom. The colors should be mixed to such a consistency, that when put on, a perfectly clear and transparent appearance may be obtained. For darker shades of oak, more yellow and red should be used in the ground-work and more burnt umber in the graining-color, adding enough of the burnt umber to make the graining-color harmonize with the ground-work. And here we would suggest that every grainer, who desires to perfect himself in the art, should procure small pieces of the various kinds of wood he wishes to imitate, and in all cases mix his colors in harmony with those shown in the wood—mixing his ground-work so as to compare with the lightest shade observable in the wood.

Too much care cannot be taken in the preparation of graining-colors; more failures have been made through neglect of this, than in the execution of the work itself, for except the colors are in proper harmony with the wood desired to be imitated, the work, though well executed, must be a failure in the production of the wished-for object.

For the last coat of the ground-work for oak, there should be a sufficiency of oil to impart a slight gloss when laid on, which enables it to be wiped clean, free, and unclouded.

For shading oak use a little raw Sienna, raw and burnt umber, mixing with oil, turpentine, japan, etc., as before mentioned. Where knots 8 or curls occur in the grain, as shown in our illustration, there light and careless shades should be thrown in, avoiding anything prominent or harsh, and in most cases make the growth or heart slightly darker than at the edge. A beautiful effect can be produced by combing over the flaking with a fine or coarse rubber comb, blending very lightly in the same direction the veins or comb take. The effect produced is to sink the flaking, making it look solid and true to nature.

For wiping out oak (as in samples shown), see description of process in our following chapter on black walnut, using the same tools, etc. (rubber combs, English or American steel combs in oak, not in walnut). Where flaking is done it is combed first with a coarse, then a fine steel comb, but where heart or growth-pieces occur, no comb should be used until wiped out, then comb with a fine comb very lightly in the same direction the grains may run.

In graining, particularly oak, care should be taken to have the grains lose themselves regularly at the sides, not leaving the heart-piece abruptly, but gradually (as shown in our illustration), preserving a proper harmony of colors from centre to outside.

9

## BLACK WALNUT.

Illustrations of WALNUT include Plates 18-28.

The same care should be taken in puttying, sand-papering, mixing, and applying, as hereinbefore suggested in the chapter upon graining oak.

The ground-work for black walnut should be mixed with pure white lead, turpentine, oil, japan, etc., colored with chrome yellow or good Rochelle ochre, American vermilion, or English Venetian red, and burnt umber, which if properly combined produces the most proper ground-work attainable. This wood varies in color, some pieces bearing upon the yellow, and others upon the red, either of which may be correctly imitated by adding yellow or red as the case requires. There are some pieces, however, of a grayish cast, and if such a characteristic is desired in graining, add to the ground-work a little Vandyke brown.

The ground-work (last coat) should be so mixed as to have, when dry, an egg-shell gloss, in order to prevent the first coat of graining (which is "distemper-color") from crawling or running together. Black walnut is a very porous wood, and unless the pores are properly shown in the graining, the imitation will be far from perfect; no grainer, therefore, should depart so far from nature as to omit this necessary and absolute consideration.

For the accomplishment of a correct imitation in this respect, take a small quantity of sour or common ale, or, if not obtainable, a little vinegar and water (equal parts) will do (urine is an excellent substitute for either of the liquids named), and to this add, for coloring purposes, three-fourths burnt umber and one-fourth Vandyke brown; when this is 10 applied, and before dry, take a dry brush (a flat one is preferable), and "whip" the color thoroughly with the same, keeping the hand close to the surface of the object to be grained; and as pores in some pieces of walnut show far more distinctly than in others, to imitate this, certain portions should be whipped very coarsely, while other portions should be whipped very fine. Care must be taken in whipping, to have all joints, etc., left perfectly square as constructed, and the whipping should invariably be done as the grain of the wood is designed to run. The distemper-color should be mixed to a thickness, that, when applied and properly whipped, the general tone of the ground-work shall not be materially changed.

Some grainers, before proceeding further in graining black walnut, have varnished the distemper-coat; we regard this as entirely useless, as well as detrimental to the general tone of the graining when done. The impression current among some painters, that when the graining-color is applied to the distemper-color, without first varnishing, it (the distemper-color) will rub up, is erroneous, for when perfectly dry it is all ready to receive the graining-color.

After complying with the foregoing directions, the article being now all ready for graining, having, as shown, received the distemper-color, take three-fourths burnt umber and one-fourth Vandyke brown, mixed with three-fourths turpentine, one-fourth oil and japan, using beeswax or soap to prevent its running as in oak-graining (of course the color must be varied to comply with the ground-work by adding burnt umber, Vandyke brown, or burnt Sienna, as hereinbefore set forth in our directions for oak-graining), and to avoid darkening the graining but a very little, the color should be used thin.

In graining a panel, for instance, in order to obtain a correct imitation of black walnut, the grainer, when running the heart-piece (as shown 11 in our illustrations), should have upon his pallet, glass, or board, a small quantity of umber and Vandyke brown to darken the centre a little, thereby showing the grains perfectly clear in the centre while they lose themselves near the outer edge.

In graining black walnut, combs should be used as little as possible, leaving all the plain parts to be finished in the glazing. For wiping out growths, some use chamois, others use cotton cloths drawn closely over the thumb nail, while many use in place of either, a small piece of rubber, or belting cut about one-fourth of an inch wide at the end used, and in some instances, where a cheap job of graining is desired, rubber combs cut fine and coarse can be used with good success in running growths or hearts by blending lightly after combing.

This brings the work up to a finishing, or shading point, for which purpose use principally Vandyke brown, burnt umber and ivory-black, mixed with oil, turpentine, etc. (as hereinbefore named), and by keeping upon the board, glass or pallet, a little of these separately, and using more of one than the other, a beautiful and correct variety can be produced, it being almost impossible to find two pieces of walnut exactly alike in shade. Like the rest, shading must be applied with a brush, and where crooks, curls, or knots in the grain may appear (see illustrations), careless and light shades should be thrown in, and in the greater number of cases cause growths a trifle darker than edges. For shading the plain parts, a fine and very proper effect will be produced by first applying the color and then by laying on a flat brush, pressing it heavily, and drawing it crooked or straight as desired, then by blending the same very lightly. Where the brush is not thus used, a similar effect can be produced by wiping out lines at small intervals, then blending, in all cases avoiding the too common error of putting too much work in the graining, and preserve a 12 proper harmony of colors so that when completed the work will appear rich, clean, and finished.

All graining can be finished by varnishing, or to imitate in "oil-finish" if preferable. Should the latter be desirable take one (1) quart of turpentine; one-fourth (1/4) lb. of white wax (melted in turpentine), adding one half (1/2) pint of best coach varnish (hard drying); one half (1/2) pint of boiled oil, and one (1) gill of japan—apply with a brush, and use sparingly, one coat is sufficient.

By conforming to our directions, in the graining of black walnut, great and satisfactory results will follow.

13

## ROSEWOOD.

Illustrations of ROSEWOOD include Plates 29-31.

In preparing work for rosewood the same instructions should be followed as are laid down in the preceding remarks upon the graining, etc., of black walnut, for the ground-work of both woods is formed of the same colors, only more of the red and yellow is used for rosewood than walnut, as the former varies more in tone between red and yellow. The same rules in both cases should be conformed with, and similar tools in applying or laying on are used. In preparing ground-work for rosewood, however, a little rose pink may sometimes be employed advantageously. Of course the egg-shell gloss must be attained after the third ground-work is laid on, in order to receive the whipping-coat properly.

Pores in rosewood being very fine, the whipping should be as fine as possible. The distemper color is made from burnt umber, a very little Vandyke brown, and a small quantity of rose-pink, ground in ale, or vinegar and water, etc., as before mentioned, and applied very thin. The first coat of graining is mixed from Vandyke brown, burnt umber, and ivory-black (though mainly from the former), ground very fine in oil, turpentine, wax, etc., and must stand after being mixed for some six hours before applying. In some cases, where a reddish cast is desired, it will be well to use a trifle more of the rose-pink.

As the grains in rosewood run very irregularly (see illustration), great care must be maintained in combing, it being necessary in most cases to employ extremely coarse and fine combs; and at times it may be absolutely necessary to use a pencil, in bringing up this imitation to perfection, and all of the combing and pencilling must be blended down very 14 softly with a fine badger blender. For the glazing, the same colors may be used, though chiefly Vandyke brown and ivory-black, making the dark places principally from the latter, though, of course, all of these colors are to be made exceedingly thin and as transparent as possible.

Where a particularly rich finish is desired, a good effect will result by giving the work another extremely thin coat of glazing, composed of rose-pink with a little ivory-black, thus sinking and harmonizing the whole work, giving it a rich and very fine appearance. When the work becomes thoroughly hard and dry, it can be finished either in varnish or oil, as heretofore mentioned in the finishing of black walnut.

15

## MAPLE.

Illustrations of MAPLE include Plates 32-34.

This, though a very beautiful wood, is not as commonly used in graining as some others, though a fine effect can be produced by graining panels, etc., in rooms where the principal graining may be black walnut, oak, or rosewood, forming thus a contrast, which, when well executed, presents an extremely fine appearance, and as maple is never used for an outside finish (therefore not being exposed to the weather), it can be grained more successfully in distemper than in oil, and also much more readily, the consequence of which is, we shall speak of it as being grained only in distemper color, though the same colors, used by a skilful hand, in oil, will produce the same beautiful effect.

The ground-work for maple is made from white, tinted with chrome yellow, making the very lightest cream, and the same rules as to mixing, laying on, etc., etc., are applicable to the graining of maple as to the other woods hereinbefore mentioned, viz., walnut, oak, and rosewood.

The graining color is made from raw Sienna and a little raw umber, not far from equal parts, and ground fine in ale, etc., as before laid down for distemper colors. By rubbing the ground-work upon which all distemper colors are laid, with a damp sponge, it will be found to take the color much more readily than when not so rubbed.

The tools necessary for the graining of maple are a badger-hair blender, two or three top, or over-grainers, varying in width; and in running of heart-pieces, pencils must be used. For making the curls in curly maple, there can be nothing better than a raw potato, cut, say two or three inches wide, with a thin, straight edge, although the work can be performed 16 by using a piece of rubber, or belting, with a similar straight edge. A flat camel's-hair brush, used wet, will accomplish the same, and for this purpose it is employed quite successfully.

In forming the bird's-eyes, a potato cut in two, near the centre, with various inequalities made upon the smooth surface, and carelessly pounced over the surface of the work, will prove successful; but we know of nothing better adapted for this purpose than the ends of the fingers, touching the surface therewith at intervals. (See samples.)

After a thin coating of the distemper is laid on, for the production of curly maple, take a potato, or some one of the other things spoken of, and form the curls by running it crosswise, making them as irregular and careless as possible, then blend them down to a perfect harmony, after which pounce the same with the end of the blender as softly and finely as possible, as the pores in maple are nearly indistinct. After allowing this to dry thoroughly, if a heart or growth is desired, run the same with a pencil as before mentioned, or form the grains by taking the over-grainer, touching it in the color (having combed the grainer before being touched in the color); then run it down over the work, holding the hand near the work; then blend those also carefully, and, especially in maple, avoid anything harsh or stiff in the color, or the running of the grains, as maple, when completed, is a very light and transparent wood. Where bird's-eye-maple is desired (after the thin distemper color has been used), take the damp sponge and roll it carelessly over the surface, which will remove a portion; then blend softly as in forming the curls, after which, and before it is allowed to dry, form the bird's-eye with a potato or fingers, as before mentioned, in those parts where the color has not been removed; then, when entirely dry, form the grains either with a pencil or a grainer, as set forth in directions on curly maple. Care should be taken to have the bird's-eyes shaded (as per illustration), thereby making them natural and complete. 17 After complying with the foregoing instructions, the work is ready for the varnish, and in most cases will be found satisfactorily finished, though it can be materially improved by first giving it a very thin coat of varnish, then a very thin glazing coat of the same colors, though principally of Sienna, forming curls, shades, etc., where they may have been omitted, or will be found to improve the work. You will observe in our illustrations that the grains of maple, both bird's-eye and curly, are entirely different from those of any other kind of wood, both in course and formation. In all cases the illustrations herein given must be followed as closely as possible, which, if properly complied with, will, in all cases, produce the desired result. If desired to be grained in oil, combs should be used instead of top, or over-grainers.

In connection with maple, we would here say that there is such a wood as satin-wood, but it is rarely used in any manner.

If, however, it should be desirable to grain it, it will be found that the colors used in graining maple (raw Sienna being the chief material) are the same as those used in the graining of satin-wood, and the process varies in no essential manner, only that the colors and graining should be more indistinct with satin-wood, it being an extremely pale and transparent wood. Care must be observed to preserve in the imitation the purity and character of the original.

18

## ASH.

Illustrations of ASH include Plates 35-38.

A very beautiful and prolific wood, attainable so easily throughout the greater part of the country, is now growing in daily favor for the interior of houses and other buildings, its susceptibility of high finish making it desirable as well as handsome, and probably when well grained it presents more attractiveness than any of the other woods.

Grainers, therefore, should become skilled as far as possible in the imitation of this brilliant and durable wood, and it seems our duty to call especial attention to our illustrations of this wood while endeavoring to impress upon the minds of our readers its adaptability for the purposes herein cited. The ground-work of ash is produced by using a little chrome or Rochelle yellow, together with the least possible tint of red, to which add a trifle of Vandyke brown. But little of this must be used or the ground-work will be too gray. The color when mixed must compare with the lightest shade found in the wood itself. The ground-work must be left with the egg-shell gloss, spoken of in our former chapters. Ash being a very porous wood, the pores, therefore, must, in no case, be left out in the graining, otherwise the work will be incomplete, and for the purpose of producing those take one-half raw umber, one-fourth raw sienna, and one-eighth Vandyke brown; grind all in ale, etc., and apply the same, using it very thin, and whipping it thoroughly, as instructed in directions pertaining to rosewood, etc.

For the second coat, or oil-graining, use the same colors in about the same quantities, ground in oil, turpentine, wax, etc., as mentioned in graining other woods. The same rules as to graining black walnut—darkening 19 the centre a little, and having the grains lose themselves at the sides or ends—are applicable in the graining of ash, and the same tools should also be used in the graining of this wood as are used in that of black walnut; the hand should run the same as in graining walnut, and the grains should run with equal regularity. In shading, the same colors may be used, adding a little more Vandyke brown, and grainers, particularly in shading, should study to imitate nature itself in each particular. Of course the colors should be so mixed and strained as to avoid the possibility of their containing harsh or lumpy substances, so that the work will prove to be clean, smooth, and free from any cloudy or impure appearance.

It can be finished in varnish, or in oil, the same as other woods heretofore named.

20

## CHESTNUT.

Illustrations of CHESTNUT include Plates 39-42.

Is largely used, and, like ash, is a particularly beautiful wood. Becoming so well and favorably known for the various purposes to which it can be applied, grainers should study well its beauties, and in their imitation thereof strive to hold the mirror up to nature. The ground-work of chestnut is produced with the same class of colors as that of ash is, only a little more Vandyke brown should be employed, to produce a more grayish tint than is found in ash.

Though chrome is used in the ground-work of chestnut, we deem it inferior to Rochelle yellow, inasmuch as the latter has a more subdued shade, in nearer conformity to chestnut, than that produced by chrome, the latter giving the work a more sprightly hue than is observable in the wood itself. Chestnut is very porous, or rather it shows a more porous condition than ash itself, and to produce this there should be used a little raw umber, raw Sienna, burnt umber, and Vandyke brown, in nearly equal parts, ground in ale, giving the work a very thin coat, and whipping coarsely, so that when done the pores will show very plainly. For the second, or oil-graining, use the same colors, in the same quantities, ground in oil, turpentine, wax, etc., as before instructed. Grain on much the same principle as in ash, only coarser,—the grains in chestnut running much coarser, but yet with the same regularity as those found either in ash or black walnut. For shading chestnut use a little burnt umber and Vandyke brown (rather more of the former), to which add a small quantity of raw Sienna, grinding them in oil, turpentine, etc. In applying this color have it very thin, as in other grainings, and as chestnut is a plain 21 wood, presenting a great uniformity of color in itself, great care must be taken to avoid any material change in the appearance of the graining by any heavy shades.

This rule, it will be observed, is in this regard dissimilar from that laid down to govern the graining of ash, as the latter presents in nature many heavy and eccentric shades, etc., while in the former there is very little diversity in the shade. The same process of wiping out and darkening the centre is applicable to this wood as that set forth to govern in the cases of walnut and ash, similar combs and tools being used in the work upon each and all; and, like the other woods, chestnut can be finished in oil or varnish, as heretofore noted, and when finished is substantial in appearance and very beautiful.

Pl. 1

OAK FLAKING.

Pl. 2

OAK GROWTH.

Pl. 3

OAK FLAKING.

Pl. 4

OAK GROWTH AND FLAKING.

Pl. 5

OAK FLAKING.

Pl. 6

OAK GROWTH.

Pl. 7

OAK FLAKING.

Pl. 8

OAK GROWTH.

Pl. 9

OAK FLAKING.

Pl. 10

OAK GROWTH.

Pl. 11

OAK FLAKING.

Pl. 12

WHITE OAK GROWTH.

Pl. 13

OAK FLAKING.

Pl. 14

WHITE OAK GROWTH.

Pl. 15

OAK FLAKING.

Pl. 16

OAK GROWTH, SHOWING KNOTS.

Pl. 17

OAK GROWTH.

Pl. 18

BLACK WALNUT GROWTH.

Pl. 19

BLACK WALNUT GROWTH.

Pl. 20

BLACK WALNUT GROWTH.

Pl. 21

BLACK WALNUT GROWTH.

Pl. 22

BLACK WALNUT GROWTH.

Pl. 23

BLACK WALNUT GROWTH.

Pl. 24

BLACK WALNUT GROWTH.

Pl. 25

BLACK WALNUT GROWTH.

Pl. 26

BLACK WALNUT GROWTH AND CROTCH.

Pl. 27

FRENCH WALNUT.

Pl. 28

FRENCH WALNUT.

Pl. 29

ROSEWOOD.

Pl. 30.

ROSEWOOD.

Pl. 31

ROSEWOOD.

Pl. 32

CURLED MAPLE.

Pl. 33

BIRDS EYE-MAPLE.

Pl. 34

CURLED MAPLE.

Pl. 35

ASH GROWTH.

Pl. 36

ASH GROWTH.

Pl. 37

ASH GROWTH.

Pl. 38

ASH GROWTH.

Pl. 39

CHESTNUT GROWTH.

Pl. 40

CHESTNUT GROWTH.

Pl. 41

CHESTNUT GROWTH.

Pl. 42

CHESTNUT GROWTH.

Transcriber's note:
The following lines which include an active link, have been inserted in order to aid the reader:
Page 6 Illustrations of OAK include Plates 1-17.
Page 9 Illustrations of WALNUT include Plates 18-28.
Page 11 Illustrations of ROSEWOOD include Plates 29-31.
Page15 Illustrations of MAPLE include Plates 32-34.
Page 18 Illustrations of ASH include Plates 35-38.
Page 20 Illustrations of CHESTNUT include Plates 39-42.

    End of the Project Gutenberg EBook of The Art of Graining: How Acquired and
    how Produced., by Charles Pickert and A. Metcalf

    *** END OF THIS PROJECT GUTENBERG EBOOK THE ART OF GRAINING ***

    ***** This file should be named 45079-h.htm or 45079-h.zip *****
    This and all associated files of various formats will be found in:
            http://www.gutenberg.org/4/5/0/7/45079/

    Produced by Chris Curnow, Mary Akers and the Online
    Distributed Proofreading Team at http://www.pgdp.net (This
    file was produced from images generously made available
    by The Internet Archive)

    Updated editions will replace the previous one--the old editions
    will be renamed.

    Creating the works from public domain print editions means that no
    one owns a United States copyright in these works, so the Foundation
    (and you!) can copy and distribute it in the United States without
    permission and without paying copyright royalties.  Special rules,
    set forth in the General Terms of Use part of this license, apply to
    copying and distributing Project Gutenberg-tm electronic works to
    protect the PROJECT GUTENBERG-tm concept and trademark.  Project
    Gutenberg is a registered trademark, and may not be used if you
    charge for the eBooks, unless you receive specific permission.  If you
    do not charge anything for copies of this eBook, complying with the
    rules is very easy.  You may use this eBook for nearly any purpose
    such as creation of derivative works, reports, performances and
    research.  They may be modified and printed and given away--you may do
    practically ANYTHING with public domain eBooks.  Redistribution is
    subject to the trademark license, especially commercial
    redistribution.

    *** START: FULL LICENSE ***

    THE FULL PROJECT GUTENBERG LICENSE
    PLEASE READ THIS BEFORE YOU DISTRIBUTE OR USE THIS WORK

    To protect the Project Gutenberg-tm mission of promoting the free
    distribution of electronic works, by using or distributing this work
    (or any other work associated in any way with the phrase "Project
    Gutenberg"), you agree to comply with all the terms of the Full Project
    Gutenberg-tm License available with this file or online at
      www.gutenberg.org/license.

    Section 1.  General Terms of Use and Redistributing Project Gutenberg-tm
    electronic works

    1.A.  By reading or using any part of this Project Gutenberg-tm
    electronic work, you indicate that you have read, understand, agree to
    and accept all the terms of this license and intellectual property
    (trademark/copyright) agreement.  If you do not agree to abide by all
    the terms of this agreement, you must cease using and return or destroy
    all copies of Project Gutenberg-tm electronic works in your possession.
    If you paid a fee for obtaining a copy of or access to a Project
    Gutenberg-tm electronic work and you do not agree to be bound by the
    terms of this agreement, you may obtain a refund from the person or
    entity to whom you paid the fee as set forth in paragraph 1.E.8.

    1.B.  "Project Gutenberg" is a registered trademark.  It may only be
    used on or associated in any way with an electronic work by people who
    agree to be bound by the terms of this agreement.  There are a few
    things that you can do with most Project Gutenberg-tm electronic works
    even without complying with the full terms of this agreement.  See
    paragraph 1.C below.  There are a lot of things you can do with Project
    Gutenberg-tm electronic works if you follow the terms of this agreement
    and help preserve free future access to Project Gutenberg-tm electronic
    works.  See paragraph 1.E below.

    1.C.  The Project Gutenberg Literary Archive Foundation ("the Foundation"
    or PGLAF), owns a compilation copyright in the collection of Project
    Gutenberg-tm electronic works.  Nearly all the individual works in the
    collection are in the public domain in the United States.  If an
    individual work is in the public domain in the United States and you are
    located in the United States, we do not claim a right to prevent you from
    copying, distributing, performing, displaying or creating derivative
    works based on the work as long as all references to Project Gutenberg
    are removed.  Of course, we hope that you will support the Project
    Gutenberg-tm mission of promoting free access to electronic works by
    freely sharing Project Gutenberg-tm works in compliance with the terms of
    this agreement for keeping the Project Gutenberg-tm name associated with
    the work.  You can easily comply with the terms of this agreement by
    keeping this work in the same format with its attached full Project
    Gutenberg-tm License when you share it without charge with others.

    1.D.  The copyright laws of the place where you are located also govern
    what you can do with this work.  Copyright laws in most countries are in
    a constant state of change.  If you are outside the United States, check
    the laws of your country in addition to the terms of this agreement
    before downloading, copying, displaying, performing, distributing or
    creating derivative works based on this work or any other Project
    Gutenberg-tm work.  The Foundation makes no representations concerning
    the copyright status of any work in any country outside the United
    States.

    1.E.  Unless you have removed all references to Project Gutenberg:

    1.E.1.  The following sentence, with active links to, or other immediate
    access to, the full Project Gutenberg-tm License must appear prominently
    whenever any copy of a Project Gutenberg-tm work (any work on which the
    phrase "Project Gutenberg" appears, or with which the phrase "Project
    Gutenberg" is associated) is accessed, displayed, performed, viewed,
    copied or distributed:

    This eBook is for the use of anyone anywhere at no cost and with
    almost no restrictions whatsoever.  You may copy it, give it away or
    re-use it under the terms of the Project Gutenberg License included
    with this eBook or online at www.gutenberg.org

    1.E.2.  If an individual Project Gutenberg-tm electronic work is derived
    from the public domain (does not contain a notice indicating that it is
    posted with permission of the copyright holder), the work can be copied
    and distributed to anyone in the United States without paying any fees
    or charges.  If you are redistributing or providing access to a work
    with the phrase "Project Gutenberg" associated with or appearing on the
    work, you must comply either with the requirements of paragraphs 1.E.1
    through 1.E.7 or obtain permission for the use of the work and the
    Project Gutenberg-tm trademark as set forth in paragraphs 1.E.8 or
    1.E.9.

    1.E.3.  If an individual Project Gutenberg-tm electronic work is posted
    with the permission of the copyright holder, your use and distribution
    must comply with both paragraphs 1.E.1 through 1.E.7 and any additional
    terms imposed by the copyright holder.  Additional terms will be linked
    to the Project Gutenberg-tm License for all works posted with the
    permission of the copyright holder found at the beginning of this work.

    1.E.4.  Do not unlink or detach or remove the full Project Gutenberg-tm
    License terms from this work, or any files containing a part of this
    work or any other work associated with Project Gutenberg-tm.

    1.E.5.  Do not copy, display, perform, distribute or redistribute this
    electronic work, or any part of this electronic work, without
    prominently displaying the sentence set forth in paragraph 1.E.1 with
    active links or immediate access to the full terms of the Project
    Gutenberg-tm License.

    1.E.6.  You may convert to and distribute this work in any binary,
    compressed, marked up, nonproprietary or proprietary form, including any
    word processing or hypertext form.  However, if you provide access to or
    distribute copies of a Project Gutenberg-tm work in a format other than
    "Plain Vanilla ASCII" or other format used in the official version
    posted on the official Project Gutenberg-tm web site (www.gutenberg.org),
    you must, at no additional cost, fee or expense to the user, provide a
    copy, a means of exporting a copy, or a means of obtaining a copy upon
    request, of the work in its original "Plain Vanilla ASCII" or other
    form.  Any alternate format must include the full Project Gutenberg-tm
    License as specified in paragraph 1.E.1.

    1.E.7.  Do not charge a fee for access to, viewing, displaying,
    performing, copying or distributing any Project Gutenberg-tm works
    unless you comply with paragraph 1.E.8 or 1.E.9.

    1.E.8.  You may charge a reasonable fee for copies of or providing
    access to or distributing Project Gutenberg-tm electronic works provided
    that

    - You pay a royalty fee of 20% of the gross profits you derive from
         the use of Project Gutenberg-tm works calculated using the method
         you already use to calculate your applicable taxes.  The fee is
         owed to the owner of the Project Gutenberg-tm trademark, but he
         has agreed to donate royalties under this paragraph to the
         Project Gutenberg Literary Archive Foundation.  Royalty payments
         must be paid within 60 days following each date on which you
         prepare (or are legally required to prepare) your periodic tax
         returns.  Royalty payments should be clearly marked as such and
         sent to the Project Gutenberg Literary Archive Foundation at the
         address specified in Section 4, "Information about donations to
         the Project Gutenberg Literary Archive Foundation."

    - You provide a full refund of any money paid by a user who notifies
         you in writing (or by e-mail) within 30 days of receipt that s/he
         does not agree to the terms of the full Project Gutenberg-tm
         License.  You must require such a user to return or
         destroy all copies of the works possessed in a physical medium
         and discontinue all use of and all access to other copies of
         Project Gutenberg-tm works.

    - You provide, in accordance with paragraph 1.F.3, a full refund of any
         money paid for a work or a replacement copy, if a defect in the
         electronic work is discovered and reported to you within 90 days
         of receipt of the work.

    - You comply with all other terms of this agreement for free
         distribution of Project Gutenberg-tm works.

    1.E.9.  If you wish to charge a fee or distribute a Project Gutenberg-tm
    electronic work or group of works on different terms than are set
    forth in this agreement, you must obtain permission in writing from
    both the Project Gutenberg Literary Archive Foundation and Michael
    Hart, the owner of the Project Gutenberg-tm trademark.  Contact the
    Foundation as set forth in Section 3 below.

    1.F.

    1.F.1.  Project Gutenberg volunteers and employees expend considerable
    effort to identify, do copyright research on, transcribe and proofread
    public domain works in creating the Project Gutenberg-tm
    collection.  Despite these efforts, Project Gutenberg-tm electronic
    works, and the medium on which they may be stored, may contain
    "Defects," such as, but not limited to, incomplete, inaccurate or
    corrupt data, transcription errors, a copyright or other intellectual
    property infringement, a defective or damaged disk or other medium, a
    computer virus, or computer codes that damage or cannot be read by
    your equipment.

    1.F.2.  LIMITED WARRANTY, DISCLAIMER OF DAMAGES - Except for the "Right
    of Replacement or Refund" described in paragraph 1.F.3, the Project
    Gutenberg Literary Archive Foundation, the owner of the Project
    Gutenberg-tm trademark, and any other party distributing a Project
    Gutenberg-tm electronic work under this agreement, disclaim all
    liability to you for damages, costs and expenses, including legal
    fees.  YOU AGREE THAT YOU HAVE NO REMEDIES FOR NEGLIGENCE, STRICT
    LIABILITY, BREACH OF WARRANTY OR BREACH OF CONTRACT EXCEPT THOSE
    PROVIDED IN PARAGRAPH 1.F.3.  YOU AGREE THAT THE FOUNDATION, THE
    TRADEMARK OWNER, AND ANY DISTRIBUTOR UNDER THIS AGREEMENT WILL NOT BE
    LIABLE TO YOU FOR ACTUAL, DIRECT, INDIRECT, CONSEQUENTIAL, PUNITIVE OR
    INCIDENTAL DAMAGES EVEN IF YOU GIVE NOTICE OF THE POSSIBILITY OF SUCH
    DAMAGE.

    1.F.3.  LIMITED RIGHT OF REPLACEMENT OR REFUND - If you discover a
    defect in this electronic work within 90 days of receiving it, you can
    receive a refund of the money (if any) you paid for it by sending a
    written explanation to the person you received the work from.  If you
    received the work on a physical medium, you must return the medium with
    your written explanation.  The person or entity that provided you with
    the defective work may elect to provide a replacement copy in lieu of a
    refund.  If you received the work electronically, the person or entity
    providing it to you may choose to give you a second opportunity to
    receive the work electronically in lieu of a refund.  If the second copy
    is also defective, you may demand a refund in writing without further
    opportunities to fix the problem.

    1.F.4.  Except for the limited right of replacement or refund set forth
    in paragraph 1.F.3, this work is provided to you 'AS-IS', WITH NO OTHER
    WARRANTIES OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO
    WARRANTIES OF MERCHANTABILITY OR FITNESS FOR ANY PURPOSE.

    1.F.5.  Some states do not allow disclaimers of certain implied
    warranties or the exclusion or limitation of certain types of damages.
    If any disclaimer or limitation set forth in this agreement violates the
    law of the state applicable to this agreement, the agreement shall be
    interpreted to make the maximum disclaimer or limitation permitted by
    the applicable state law.  The invalidity or unenforceability of any
    provision of this agreement shall not void the remaining provisions.

    1.F.6.  INDEMNITY - You agree to indemnify and hold the Foundation, the
    trademark owner, any agent or employee of the Foundation, anyone
    providing copies of Project Gutenberg-tm electronic works in accordance
    with this agreement, and any volunteers associated with the production,
    promotion and distribution of Project Gutenberg-tm electronic works,
    harmless from all liability, costs and expenses, including legal fees,
    that arise directly or indirectly from any of the following which you do
    or cause to occur: (a) distribution of this or any Project Gutenberg-tm
    work, (b) alteration, modification, or additions or deletions to any
    Project Gutenberg-tm work, and (c) any Defect you cause.

    Section  2.  Information about the Mission of Project Gutenberg-tm

    Project Gutenberg-tm is synonymous with the free distribution of
    electronic works in formats readable by the widest variety of computers
    including obsolete, old, middle-aged and new computers.  It exists
    because of the efforts of hundreds of volunteers and donations from
    people in all walks of life.

    Volunteers and financial support to provide volunteers with the
    assistance they need are critical to reaching Project Gutenberg-tm's
    goals and ensuring that the Project Gutenberg-tm collection will
    remain freely available for generations to come.  In 2001, the Project
    Gutenberg Literary Archive Foundation was created to provide a secure
    and permanent future for Project Gutenberg-tm and future generations.
    To learn more about the Project Gutenberg Literary Archive Foundation
    and how your efforts and donations can help, see Sections 3 and 4
    and the Foundation information page at www.gutenberg.org

    Section 3.  Information about the Project Gutenberg Literary Archive
    Foundation

    The Project Gutenberg Literary Archive Foundation is a non profit
    501(c)(3) educational corporation organized under the laws of the
    state of Mississippi and granted tax exempt status by the Internal
    Revenue Service.  The Foundation's EIN or federal tax identification
    number is 64-6221541.  Contributions to the Project Gutenberg
    Literary Archive Foundation are tax deductible to the full extent
    permitted by U.S. federal laws and your state's laws.

    The Foundation's principal office is located at 4557 Melan Dr. S.
    Fairbanks, AK, 99712., but its volunteers and employees are scattered
    throughout numerous locations.  Its business office is located at 809
    North 1500 West, Salt Lake City, UT 84116, (801) 596-1887.  Email
    contact links and up to date contact information can be found at the
    Foundation's web site and official page at www.gutenberg.org/contact

    For additional contact information:
         Dr. Gregory B. Newby
         Chief Executive and Director
         gbnewby@pglaf.org

    Section 4.  Information about Donations to the Project Gutenberg
    Literary Archive Foundation

    Project Gutenberg-tm depends upon and cannot survive without wide
    spread public support and donations to carry out its mission of
    increasing the number of public domain and licensed works that can be
    freely distributed in machine readable form accessible by the widest
    array of equipment including outdated equipment.  Many small donations
    ($1 to $5,000) are particularly important to maintaining tax exempt
    status with the IRS.

    The Foundation is committed to complying with the laws regulating
    charities and charitable donations in all 50 states of the United
    States.  Compliance requirements are not uniform and it takes a
    considerable effort, much paperwork and many fees to meet and keep up
    with these requirements.  We do not solicit donations in locations
    where we have not received written confirmation of compliance.  To
    SEND DONATIONS or determine the status of compliance for any
    particular state visit www.gutenberg.org/donate

    While we cannot and do not solicit contributions from states where we
    have not met the solicitation requirements, we know of no prohibition
    against accepting unsolicited donations from donors in such states who
    approach us with offers to donate.

    International donations are gratefully accepted, but we cannot make
    any statements concerning tax treatment of donations received from
    outside the United States.  U.S. laws alone swamp our small staff.

    Please check the Project Gutenberg Web pages for current donation
    methods and addresses.  Donations are accepted in a number of other
    ways including checks, online payments and credit card donations.
    To donate, please visit:  www.gutenberg.org/donate

    Section 5.  General Information About Project Gutenberg-tm electronic
    works.

    Professor Michael S. Hart was the originator of the Project Gutenberg-tm
    concept of a library of electronic works that could be freely shared
    with anyone.  For forty years, he produced and distributed Project
    Gutenberg-tm eBooks with only a loose network of volunteer support.

    Project Gutenberg-tm eBooks are often created from several printed
    editions, all of which are confirmed as Public Domain in the U.S.
    unless a copyright notice is included.  Thus, we do not necessarily
    keep eBooks in compliance with any particular paper edition.

    Most people start at our Web site which has the main PG search facility:

         www.gutenberg.org

    This Web site includes information about Project Gutenberg-tm,
    including how to make donations to the Project Gutenberg Literary
    Archive Foundation, how to help produce our new eBooks, and how to
    subscribe to our email newsletter to hear about new eBooks.